From Corby Dawson Sat Feb 28 17:02:52 2009 To: time-nuts@febo.com
Well after re-researcing the pinouts again I decided to post this while they are fresh.
These Pinouts are for units removed from FTS Cesium standards and were verified by measurement in the standard.

PIN	1000B			1000A-100		1200			9110

1	EFC ground		EFC ground		EFC ground		EFC ground

2	EFC +- 10V		EFC +- 10V		EFC 0 to +10V 	EFC 0 to +10V

3	coarse tune wiper 	NC 			NC 			NC

4	+12 pot ref. (10K)	NC 			NC 			NC

5	Ground 		Ground 		Ground 		Ground

6	oven mon. 		oven mon. 		oven mon.		oven mon.

7	+28V oven 		+18V oven 		NC 			NC

8	+28V elect. 		+28V 			+28V 			+28V

9	case ground 		NC 			NC 			NC

Hope this will help others!

Corby Dawson